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PANTHER DC
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FEATURES
• STURDY STRUCTURE
• EASY TO INSTALL
• COMPACT DESIGN
• IP55


The PANTHER DC is a rotary, self-priming vane pump suitable for all applica- tions in which important flow rates are required. This equipment is fitted with an incorporated filter (100Μ) and by-pass valve. The 24/12 V version can be used with both voltages.

























PERFORMANCE

UP TO
70 L/MIN

FLOW-RATE


30 MIN

DUTY CICLE




12/24V
VOLTAGE
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